{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["维修工程量清单"],"read":"whole","date_system":"1900"}

{"sheet":"维修工程量清单","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"merged":[[0,0,2,7],[8,0,8,7]]}
["四川省残疾人体育训练中心部分基础设施维修改造项目工程量清单（报价单）"]
[]
[]
["序号","项目名称","特征描述","单位","工程量","综合单价（元）","合计（元）","备注说明"]
[1,"宿舍楼卫生间、卧室及通道改造约9㎡/间","1.拆除墙瓷砖粘接层\n2.拆除坐便器\n3.拆移木门（利旧）\n4.拆除已损木地板\n5.拆除建渣搬运及处理\n6.墙地面防水:K11+辅料\n7.防水保护层:水泥砂浆保护层\n8.铺装400*800墙砖，铺装400*400地砖\n9.安装原木吊门\n10.更换已损坏木地板\n11.更换不锈钢地漏/2个                    \n13.坐便器利旧安装\n14.更换已损坏木地板\n15.修补墙面乳胶漆","间",56]
[2,"康复理疗室进行开窗通风，开窗面积约3㎡/扇","1.拆除原有玻璃窗\n2.安装定制86推拉窗（lowe玻璃）\n3.安装定制平开窗（lowe玻璃）\n4.安装定制纱窗\n5.施工垃圾自行运走","扇",2]
[3,"停车场增加遮阳车棚面积约63㎡","1.基础施工：挖基坑安制预埋件、浇筑混凝土\n2.棚体搭建：骨架采用不锈钢矩管结构，顶棚采用4mm树脂瓦\n3.施工垃圾自行运走","平方米",63]
[4,"合计"]
["说明：报价包含人工、材料、安装、运输、装卸、售后服务、税费等费用，即交付采购人使用前所有可能发生的费用。"]